

[bookmark: _8yaejbiaz9q8]Internal battery NB (7.2V/190Ah)
[bookmark: _sp8hkg1mwizf]Pack of 20 non-rechargeable LTC ER34615 batteries to install in a compatible Ajax casing
	Battery type
	Battery
20 × ER34615
Non-rechargeable lithium thionyl chloride battery with a HPC-1520 pulse capacitor.

Nominal voltage
7.2 V⎓

Nominal capacity
190 Ah
At a current consumption of 10 mA (with Battery power saver mode enabled), a temperature of 25 °C 77 °F, and correct placement of the battery in the Ajax casing. Low temperatures may reduce battery capacity and shorten the battery life.

Maximum load current
700 mA

End-of-life battery voltage
4 V⎓

	Cautions
	Do not short the power terminals.
Do not recharge the battery.
Use the battery only with compatible devices.
The battery is designed for indoor use only.
Secure the battery in the casing using the hook-and-loop fastener (included in the Case D (430) and Case E (395) complete sets).

	Product
	Dimensions
182 × 124 × 64 mm
7.17″ × 4.88″ × 2.52″

Weight
2.1 kg
4.63 lb

Battery connector type
Molex 2139-2 or equivalent

Operating temperature range
from −25 °C to +65 °C
from −13 °F to 149 °F

Operating relative humidity
from 40% to 80%

	Complete set
	Internal battery NB (7.2V/190Ah)

	Warranty
	24 months





