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[bookmark: _eeqh4xq96b0v]Pack of 78 rechargeable LiFePO4 batteries to install in a compatible Ajax casing

	Battery type
	Battery
78 × IFR18650
Rechargeable lithium iron phosphate (LiFePO4) battery cells.

Battery configuration
2S39P

Nominal voltage
6.4 V⎓

Nominal capacity
78 Ah

Maximum charge current
15 A
Via the battery charging connector.

TVC (Terminal Voltage Control)
7.2 V⎓ (3.6 V⎓ per cell)

Maximum discharge current
2 A
Via the connector for attaching the battery to the hub.

Discharge cut-off voltage
4.5 V⎓

	Charging and discharging parameters
	Charging temperature range
from 0 °C to +45 °C
from 32 °F to 113 °F

Charging relative humidity
60 ± 25%

Discharging temperature range
from −25 °C to +65 °C
from −13 °F to 149 °F

Discharging relative humidity
60 ± 25%

	Storage conditions
	Storage temperature range
from −20 °C to +45 °C
from −4 °F to 113 °F

Storage humidity
60 ± 25%

	Transportation and shipping
	Shipping voltage
6.0–6.4 V⎓

Transportation requirements
For air transportation, lithium batteries must be charged to no more than 30% of their rated capacity. The shipping voltage complies with this requirement.

For other types of transportation, the battery must be handled in accordance with applicable regulations and carrier requirements.

	Cautions
	Do not expose the battery to open flames, sparks, or any other ignition source.
Do not short the power terminals.
Do not disassemble or deform the battery.
Avoid excessive mechanical impact or vibration.
Use the battery only with compatible devices.
The hub does not charge this battery. Charge the battery using a dedicated external charger. Recharge the battery every six months during storage.
The battery must be installed fully charged.
Secure the battery in the casing using the hook-and-loop fastener (included in the Case D (430) and Case E (395) complete sets).

	Product
	Dimensions
254 × 134 × 52 mm
10.00″ × 5.27″ × 2.05″

Weight
3.51 kg
7.74 lb

Battery charging connector
XT60 or equivalent

Connector for attaching the battery to the hub
Molex 2139-2 or equivalent

Operating temperature range
from −25 °C to +65 °C
from −13 °F to 149 °F

Operating relative humidity
60 ± 25%

	Complete set
	Internal battery RB (6.4V/78Ah)

	Warranty
	24 months





