[bookmark: _nfmxxg3grydf]EN54 Internal Battery (72h)
[bookmark: _6r6tpgm0150y]Rechargeable Li-ion battery (7.4 V/10 Ah) to install into EN54 Fire Hub Jeweller or EN54 Fire ReX Jeweller
	Battery type
	Battery
8 × 18650
Rechargeable Li-ion battery.

Nominal voltage
7.4 V⎓

Capacity
10 Ah

	[bookmark: _sktc2zke3jt6]Power supply
	Maximum load current
3.2 A

End-of-life battery voltage
6 V⎓

	[bookmark: _ell3ymsrwzqs]Recommendations
	Use the battery with compatible devices only.

The battery is designed for indoor use only.

	[bookmark: _m4syygbom1ma]Enclosure
	Dimensions
166 × 87 × 23 mm
6.54" × 3.43" × 0.92"

Weight
443 g
15.63 oz

Operating temperature range
from −10 °C to +40 °C
from 14 °F to 104 °F

Operating humidity
up to 75% non-condensing

Protection class
IP20

	Color
	Black
White

	Complete set
	EN54 Internal Battery (72h)

	Warranty
	24 months



