[bookmark: _14avmrage121]EN54 FireProtect (Sounder/VAD) Jeweller
[bookmark: _50hywjyc9j3z]Wireless fire alarm sounder combined with a visual alarm device (VAD)
	[bookmark: _6bus8a7sk0dj]Communication
	Jeweller communication technology
Proprietary wireless communication technology to transmit commands, alarms, and events.

Key features:
· Two-way communication.
· Advanced sabotage protection.
· Block encryption featuring a dynamic key.
· Instant notifications.
· Remote control and configuration in Ajax apps.


Frequency bands
866.0–866.5 MHz
868.0–868.6 MHz
868.7–869.2 MHz
905.0–926.5 MHz
915.85–926.5 MHz
921.0–922.0 MHz
Depends on the sales region.

Maximum effective radiated power (ERP)
up to 20 mW
Automatic power control to reduce power consumption and radio interference.

Radio signal modulation
GFSK

Radio communication range
up to 1,700 m
up to 5,550 ft
Between the device and control and indicating equipment (CIE) or a range extender in an open space.

Encrypted communication
All stored and transmitted data is protected by block encryption featuring a dynamic key.

Frequency hopping
To prevent radio interference and jamming.

	[bookmark: _d7z6sy8r1xfh]Key features
	Alarm type
acoustic and light
A sounder and LED frame.

Sound volume
from 65 to XX dB at a distance of 1 m 3.3 ft
Adjusted by a PRO or user with admin rights in an Ajax app.

Sound pattern
32 tones
Learn more >

Flash frequency
90 ms ON / 1,910 ms OFF (cycle duration: 2,000 ms; frequency: 0.5 Hz)

Alarm annunciation test
To check the sound and visual alarm signals to ensure fire alarm signals are clearly audible and visible in the premises.

	[bookmark: _oe780vmb5ngh]Installation recommendations
	The device's recommended installation height is up to 3 m on the ceiling and up to 2.4 m on the wall.
The device's recommended installation height is up to 9.8 ft on the ceiling and up to 7.8 ft on the wall.

The device is designed for outdoor and indoor use.

	[bookmark: _d7z6sy8r1xfh]Sabotage protection
	Tamper alarm
Notifications of attempts to detach the device from the surface or remove the mounting panel.

Lock for SmartBracket
to secure the device on the SmartBracket mounting panel
When locked, the lock secures the device and prevents it from being removed without a special tool.

Protection against spoofing
device authentication

Connection loss detection
after 36 s
Detection time depends on Jeweller settings.

	[bookmark: _d7z6sy8r1xfh]Power supply
	Battery
4 × CR123A
Pre-installed.

Tool-free battery replacement
To replace the batteries, turn the battery compartment cover counterclockwise.
Learn more

Reverse polarity protection
Prevents device damage if the batteries are put in incorrectly.

Recommended battery type
Huiderui CR123A; 3 V; 1,600 mAh, LiMnO₂

Calculated battery life
up to 5 years
In standby mode.
up to XX minutes
In annunciation mode.

	[bookmark: _d7z6sy8r1xfh]Enclosure
	Dimensions
145 × 145 × 51 mm
5.71" × 5.71" × 2.00"

Weight
561 g
1.237 lb

Operating temperature range
from –10 °C to +50 °C
from 14 °F to 122 °F

Operating humidity
up to 80%

Protection class
IP54

	[bookmark: _d7z6sy8r1xfh]Color
	Black
White
Red


	[bookmark: _d7z6sy8r1xfh]Complete set
	EN54 FireProtect (Sounder/VAD) Jeweller
4 × CR123A battery (pre-installed)
Installation kit
Quick start guide

	Warranty
	24 months



