


[bookmark: _b4ys2rul9eon]GlandBox
[bookmark: _c2qnfzedsug2]Wiring accessory for control and indicating equipment (CIE)
	[bookmark: _jmg2tnblrz71]Key features
	Places to install cable glands
16
For routing cables that are not hidden inside the wall. There are four places on each side.

Cable gland diameter
up to 20 mm
Cable glands are not included in the complete set.

Recesses for drilling
The drill bit is fixed in the recess and does not move during drilling. We recommend using a hole saw for plastic with a diameter of up to 20 mm.

Sabotage protection
tamper button
The perforated part of GlandBox is used for the EN54 Fire Hub Jeweller tamper button to trigger when the CIE is installed in GlandBox. An Ajax system sends fault notifications if an attempt is made to detach GlandBox from the surface or remove the CIE from the mounting panel.

Cable fasteners 
To hold the cables together with ties.

Aids for easy installation
· Bubble level
· UP key
· CIE center marking
The bubble level allows for checking the casing inclination angle. The intersection of two lines marks the center of the CIE, and the UP key marks its top.



	[bookmark: _7icjp36h6bp5]Recommendations
	The accessory is designed for indoor use only.
GlandBox is compatible only with EN54 Fire Hub Jeweller.

	[bookmark: _g074uxq3mm3x]Product
	Dimensions
263 × 223 × 40 mm
10.35" × 8.78" × 1.58"

Weight
335 g
11.82 oz

Operating temperature range
from –10 °C to +40 °C
from 14 °F to 104 °F

Operating humidity
up to 75% non-condensing

Flammability rating
UL 94 V-0

	Color
	Black
White


	Complete set
	GlandBox
Installation kit
Quick start guide

	Warranty
	24 months
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