[bookmark: _278d1i6sz1zi]CurtainCam Outdoor HighMount (PhOD) Jeweller
[bookmark: _7ut8ijmodsdx]Wireless dual-technology curtain motion detector with extended photo verification possibilities. For outdoor installation at a height of 2–4 m.
	[bookmark: _fotuxs7cxayz]Communication
	Jeweller communication technology
Proprietary wireless communication technology to transmit commands, alarms, and events.

Key features:
· Two-way communication.
· Advanced sabotage protection.
· Block encryption featuring a dynamic key.
· Instant notifications.
· Remote control and configuration in Ajax apps.

Frequency bands
866.0–866.5 MHz
868.0–868.6 MHz
868.7–869.2 MHz
905.0–926.5 MHz
915.85–926.5 MHz
921.0–922.0 MHz
Depends on the sales region.

Maximum effective radiated power (ERP)
up to 25 mW
Automatic power control to reduce power consumption and radio interference.

Radio signal modulation
GFSK

Radio communication range
up to 1,700 m
up to 5,550 ft
Between the device and a hub (or a range extender) in open space.

Encrypted communication
All stored and transmitted data is protected by block encryption featuring a dynamic key.

Frequency hopping
To prevent radio interference and jamming.

Wings communication technology
Proprietary wireless communication technology to transmit large data packets.

Key features:
· Two-way communication.
· Advanced sabotage protection.
· Block encryption featuring a dynamic key.
· Data packet reload in case of transmission errors.
· Photo delivery check.

Frequency bands
866.0–866.5 MHz
868.0–868.6 MHz
868.7–869.2 MHz
905.0–926.5 MHz
915.85–926.5 MHz
921.0–922.0 MHz
Depends on the sales region.

Radio communication range
up to 1,700 m
up to 5,550 ft
Between the device and a hub (or a range extender) in open space.

Encrypted communication
All stored and transmitted data is protected by block encryption featuring a dynamic key.

Frequency hopping
To prevent radio interference and jamming.

	Detection
[bookmark: _pg1dbhjoia4l] 
	Sensitive elements
2 × PIR sensor
1 × K-band microwave sensor
Operating frequency: 24 GHz.

Motion detection distance
up to 15 m
up to 49 ft
When installed at a height of 2–4 m.
When installed at a height of 6.6–13.1 ft.
Depends on the sensitivity level adjusted in the device settings.

Main motion detection zone angles
horizontal: 7°
vertical: 73°

Pre-alarm motion detection zone angles
horizontal: 43°
vertical: 88°
To catch an intruder on photos, the device can start taking photos when a threat is detected in the pre-alarm detection zone. However, the device does not raise an alarm if the intruder never crosses the main detection zone.

Motion detection speed
from 0.3 to 2.0 m/s
from 1.0 to 6.6 ft/s
The detector sensors should be directed perpendicular to the expected intrusion path into the facility.

Sensitivity
3 levels
Adjusted by a PRO or a user with admin rights in Ajax apps.

False alarm prevention
SmartDetect
Software algorithm.

Temperature compensation
Effective motion detection at temperatures from −25 °C to +60 °C.
Effective motion detection at temperatures from −13 °F to 140 °F.

	[bookmark: _fklaiz5txixj]Photo verification
	Photo by alarm
The built-in camera activates if the detector is armed and motion is detected.

Photo on demand
A user takes pictures at any time or when the detector is armed (depending on settings). The feature is disabled by default.

Photo by scenario
The detector takes pictures automatically when other Ajax detectors are triggered. The feature is not configured by default.

Photo by schedule
The detector automatically takes photos at the specified time. The feature is not configured by default.

Photo by arming/disarming
The detector automatically takes photos when the security state is changed.

Adjustable photo resolution
640 × 480 px
320 × 240 px (by default)
Adjusted by a PRO or a user with admin rights in Ajax apps.

Camera viewing angles
horizontal: 121°
vertical: 92.5°

HDR image
Improves detail accuracy in bright and dark scenes.

IR illumination
To take photos in low-light conditions.

Series of pictures
from 1 to 5 images with a resolution of 320 × 240 px
from 1 to 3 images with a resolution of 640 × 480 px
Adjusted by a PRO or a user with admin rights in Ajax apps.

Photo delivery time
up to 9 s for 320 × 240 px resolution
up to 20 s for 640 × 480 px resolution
Photo delivery time depends on the image resolution selected in the device settings.

	[bookmark: _gsya6cd548iv]Recommendations
	It is recommended to install the detector at a height of 2–4 m.
It is recommended to install the detector at a height of 6.6–13.1 ft.

The Pet immunity feature is not available for this device.

The device is designed for outdoor and indoor use.

	Sabotage protection
	Tamper alarm
Notifications of attempts to remove the detector from the mounting panel.

Magnetometer
detects attempts to tilt or shift the detector or detach it from the surface

Anti-masking system
detects attempts to block the detector view

Holding screw
secures the device to SmartBracket

Protection against spoofing
device authentication

Communication loss detection
after 36 s
Detection time depends on the Jeweller or Jeweller/Fibra settings.

	Main power supply
	Battery
6 × CR123A
Pre-installed.

Type
type C

Calculated battery life
up to 3 years

Operating voltage range
3.8−6.5 V⎓

Nominal operating voltage
6 V⎓

Quiescent current consumption at nominal voltage
45 μA

Maximum current consumption at nominal voltage
1,200 mA

Full battery capacity
4,800 mAh

Low battery voltage
4.2 V⎓

Low battery recovery voltage
5.0 V⎓

End-of-life battery voltage
3.8 V⎓
The device switches off.

End-of-life battery capacity
300 mAh

Manufacturer
Huiderui

	[bookmark: _hoaqobbw0nvc]Optional power supply
	External supply operating voltage
12−24 V⎓
The batteries serve as a backup when an external power supply is connected.

	Enclosure
	Dimensions with the swivel mount
234 × 98 × 275 mm
9.21" × 3.86" × 10.83"

Dimensions without the swivel mount
234 × 98 × 137 mm
9.21" × 3.86" × 5.39"

Weight with the swivel mount
1,109 g
2.44 lb

Weight without the swivel mount
620 g
1.37 lb

Operating temperature range
from −25 °C to +60 °C
from −13 °F to 140 °F

Operating humidity
up to 95%

Protection class
IP55

	Color
	White


	Complete set
	CurtainCam Outdoor HighMount (PhOD) Jeweller
6 × CR123A battery (pre-installed)
SmartBracket mounting panel
Swivel mount
Hood
Installation kit
Quick start guide

	[bookmark: _jk6dcih24itj]Warranty
	24 months



