[bookmark: _y4ffti64p3y6]EN54 Internal Battery (24h)
[bookmark: _r4vvliswqk8n]Rechargeable Li-ion battery (7.4 V/5 Ah) to install into EN54 Fire Hub Jeweller or EN54 Fire ReX Jeweller
	Battery type
	Battery
4 × 18650
Rechargeable Li-ion battery.

Nominal voltage
7.4 V⎓

Capacity
5 Ah

	[bookmark: _5rkf6whlcylg]Power supply
	Maximum load current
3.2 A

End-of-life battery voltage
6 V⎓

	[bookmark: _rx3lmeb77qt1]Recommendations
	Use the battery with compatible devices only.

The battery is designed for indoor use only.

	[bookmark: _y8mth650zb2b]Enclosure
	Dimensions
166 × 87 × 23 mm
6.54" × 3.43" × 0.92"

Weight
270 g
9.52 oz

Operating temperature range
from −10 °C to +40 °C
from 14 °F to 104 °F

Operating humidity
up to 75% non-condensing

Protection class
IP20

	Color
	Black
White

	Complete set
	EN54 Internal Battery (24h)

	Warranty
	24 months



